**STEINEL Professional Presence detector**

**HF 360-2**

**BT IPD (Slave) - surface**

Type: Presence detector; Dimensions (L x W x H): 57 x 123 x 123 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,5 W; Sensor Technology: High frequency; Application, place: Indoors; Installation site: ceiling; Installation: Surface wiring; Mounting height: 2,50 – 4,00 m; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Reach, detail: 1 or 2 detection directions can be masked out by stickers for adjustment to the room situation.; HF-system: 5,8 GHz; Detection angle: 360 °; Angle of aperture: 140 °; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Detection: also through glass, wood and stud walls; Twilight setting TEACH: No; Constant-lighting control: No; Basic light level function: No; Settings via: Bluetooth; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave; IP-rating: IP54; Material: Plastic; Ambient temperature: -25 – 50 °C; Application, room: function room / ancillary room, kitchenette, stairwell, WC / washroom, Indoors; Colour: white; Colour, RAL: 9003; Manufacturer's Warranty: 5 years; Version: BT IPD (Slave) - surface; PU1, EAN: 4007841064426

**Manufacturer** Steinel

**Prod. No.** 064426

**Ordering designation**

Deliver, install and set ready for operation