**STEINEL Professional Motion detector**

**IS D360**

**white**

Type: Motion detectors; Dimensions (Ø x H): 83 x 82 mm; Mains power supply: 230 – 240 V / 50 Hz; Sensor Technology: passive infrared; Application, place: Indoors; Installation site: ceiling; Installation: In-ceiling installation; Mounting height: 2,50 – 4,00 m; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 16 m (201 m²); Detection angle: 360 °; Angle of aperture: 180 °; Switching zones: 720 switching zones; Optimum mounting height: 2,5 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Twilight setting TEACH: No; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 20 min; Output: 1000 W; Switching output 1, resistive: 1000 W; Fluorescent lamps, electronic ballast: 750 W; Fluorescent lamps, uncorrected: 500 VA; Fluorescent lamps, series-corrected: 900 VA; Switching output 1, low-voltage halogen lamps: 1000 VA; LED lamps < 2 W: 16 W; LED lamps > 2 W < 8 W: 64 W; LED lamps > 8 W: 64 W; Capacitive load in μF: 88 µF; Constant-lighting control: No; Basic light level function: No; Settings via: Potentiometers; With remote control: No; Interconnection: Yes; Type of interconnection: Master/master; IP-rating: IP20; Material: Plastic; Ambient temperature: -20 – 50 °C; Application, room: corridor / aisle, function room / ancillary room, WC / washroom, Indoors; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: white; PU1, EAN: 4007841601317

**Manufacturer** Steinel

**Prod. No.** 601317

**Ordering designation**

Deliver, install and set ready for operation