**STEINEL Professional Sensor-switched outdoor light**

**L 400 S**

**black**

Dimensions (L x W x H): 250 x 215 x 336 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Mounting height max.: 6,00 m; Sensor Technology: passive infrared; Output: 60 W; Interconnection: No; Slave modeselectable: No; With lamp: No; Lamp: All-purpose lamp; Base: E27; With motion detector: Yes; Detection angle: 240 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: r = 3 m (19 m²); Reach, tangential: r = 12 m (302 m²); Photo-cell controller: Yes; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Soft light start: Yes; Continuous light: selectable, 4h; Impact resistance: IK03; IP-rating: IP44; Protection class: II; Ambient temperature: -20 – 40 °C; Housing material: Plastic; Cover material: Glass transparent; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; Cover material: shrouds; Version: black; PU1, EAN: 4007841611019

**Manufacturer** Steinel

**Prod. No.** 611019

**Ordering designation**

Deliver, install and set ready for operation