**STEINEL Professional Sensor-switched LED outdoor light**

**DL Vario Quattro PRO LED**

**warm white anthracite**

Dimensions (Ø x H): 310 x 69 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Mounting height max.: 6,00 m; Sensor Technology: passive infrared; Output: 14 W; Interconnection: Yes; Fluorescent lamps, electronic ballast: 500 W; Fluorescent lamps, uncorrected: 500 VA; Fluorescent lamps, series-corrected: 500 VA; Fluorescent lamps, parallel-corrected: 500 VA; Switching output 1, low-voltage halogen lamps: 500 VA; LED lamps < 2 W: 16 W; LED lamps > 2 W < 8 W: 64 W; LED lamps > 8 W: 64 W; Capacitive load in μF: 88 µF; Type of interconnection: Master/master; Interconnection, number: 10 lights max.; Slave modeselectable: No; Luminous flux: 1430 lm; Efficiency: 102 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Colour Rendering Index CRI: 80-89; With lamp: Yes, STEINEL LED system; Lamp: LED cannot be replaced; LED life expectancy (max. °C): 50000 h; LED life expectancy (25 °C): > 60000 h; Base: without; LED cooling system: Passive Thermo Control; With motion detector: Yes; Detection angle: 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: No; Mechanical scalability: Yes; Reach, detail: Reach adjustable from 2 - 8 m in 4 directions (90° in each); Reach, radial: 6 x 6 m (36 m²); Reach, tangential: 16 x 16 m (256 m²); Photo-cell controller: Yes; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 30 min; Basic light level function: Yes; Basic light level function time: 10/30 min, all night; Soft light start: Yes; Continuous light: selectable, 4h; Impact resistance: IK07; IP-rating: IP54; Protection class: II; Ambient temperature: -20 – 35 °C; Housing material: Plastic; Cover material: Plastic, structured; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; Version: warm white anthracite; PU1, EAN: 4007841057596

**Manufacturer** Steinel

**Prod. No.** 057596

**Ordering designation**

Deliver, install and set ready for operation