**STEINEL Professional Sensor-switched indoor light**

**RS 10 L**

Dimensions (Ø x H): 280 x 110 mm; Mains power supply: 230 – 240 V / 50 Hz; Sensor Technology: High frequency; Transmitter power: < 1 mW; HF-system: 5,8 GHz; Output: 75 W; Power consumption: 1,1 W; Switching output 1, resistive: 800 W; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Cable; With lamp: No; Lamp: All-purpose lamp; Base: E27; With motion detector: Yes; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 160 °; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 8 m (50 m²); Continuous light: selectable; Photo-cell controller: Yes; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 15 min; Basic light level function: No; Soft light start: No; Impact resistance: IK03; IP-rating: IP44; Protection class: II; Ambient temperature: -20 – 40 °C; Housing material: Aluminium; Cover material: Glass opal; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; Installation site: wall, ceiling; PU1, EAN: 4007841730512

**Manufacturer** Steinel

**Prod. No.** 730512

**Ordering designation**

Deliver, install and set ready for operation