**STEINEL Professional Presence detector**

**IR Quattro SLIM XS**

**KNX - round V2**

Type: Presence detector; Dimensions (Ø x H): 94 x 49 mm; Power supply, detail: KNX bus; Sensor Technology: passive infrared; Application, place: Indoors; Application, place, room: one-person office, hotel room, care room, function room / ancillary room, WC / washroom, Indoors; Installation site: ceiling; Installation: Concealed wiring; Electronic scalability: No; Mechanical scalability: No; Mounting height: 2,50 – 4,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Reach, detail: Retina lens and hexagonal Fresnel structure; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 4 x 4 m (16 m²); Reach, presence: 4 x 4 m (16 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 60 s – 60 min; Basic light level function: Yes; Basic light level function in per cent: 10 – 50 %; Basic light level function time: Permanently ON, 1-255 min, all night; Basic light level function percentage, from: 10 %; Basic light level function percentage, up to: 50 %; KNX functions: Light output 4x, Presence output, Light level, Constant-lighting control, Basic light level function, HVAC output; With bus coupling: Yes; Settings via: ETS software, Remote control, Bus, Smart Remote; Interconnection: Yes; Type of interconnection: Master/slave, Master/master; IP-rating: IP20; Material: Plastic; Ambient temperature: 0 – 40 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: KNX - round; PU1, EAN: 4007841035228

**Manufacturer** Steinel

**Prod. No.** 035228

**Ordering designation**

Deliver, install and set ready for operation