**STEINEL Professional Sensor-switched LED indoor light**

**RS PRO LED Q1**

**warm white silver**

Dimensions (L x W x H): 56 x 331 x 331 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Sensor Technology: High frequency; Transmitter power: < 1 mW; HF-system: 5,8 GHz; Output: 26 W; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: Wireless; Luminous flux: 2350 lm; Colour temperature: 3000 K; Colour variation LED: SDCM3; Colour Rendering Index: 80-89; With lamp: Yes, STEINEL LED system; Lamp: LED cannot be replaced; LED life expectancy (max. °C): 50000 h; Drop in luminous flux in accordance with LM80: L70B10; Base: without; LED cooling system: Passive Thermo Control; With motion detector: Yes; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 160 °; Capability of masking out individual segments: Yes; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 8 m (50 m²); Continuous light: selectable; Photo-cell controller: Yes; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Basic light level function time: 10/30 min, all night; Main light adjustable: 50 - 100 %; Functions: Group parameterisation, Manual ON / ON-OFF, Master/slave override, Neighbouring-group function; Soft light start: Yes; Impact resistance: IK03; IP-rating: IP20; Protection class: II; Ambient temperature: -10 – 50 °C; Housing material: Aluminium; Cover material: Plastic, opal; Manufacturer's Warranty: 5 years; Settings via: DIP switches, Potentiometers, Remote control, Smart Remote; With remote control: No; Installation site: wall, ceiling; Version: warm white silver; PU1, EAN: 4007841007126

**Manufacturer** Steinel

**Prod. No.** 007126

**Ordering designation**

Deliver, install and set ready for operation