**STEINEL Professional Motion detector**

**IS 2360-3 ECO**

**black**

Type: Motion detectors; Dimensions (Ø x H): 121 x 57 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,56 W; Sensor Technology: passive infrared; Application, place: Outdoors, Indoors; Installation site: ceiling; Installation: Surface wiring; Mounting height: 2,50 – 6,00 m; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 24 m (452 m²); Detection angle: 360 °; Angle of aperture: 90 °; Switching zones: 972 switching zones; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Twilight setting TEACH: No; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 8 pcs.; Switching output 1, floating: No; Switching output 1, low-voltage halogen lamps: 1000 VA; Constant-lighting control: No; Basic light level function: No; Settings via: Potentiometers; With remote control: No; Interconnection: Yes; Type of interconnection: Master/master; IP-rating: IP54; Material: Plastic; Ambient temperature: -20 – 50 °C; Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, WC / washroom, multi-storey / underground car park, outdoors, warehouse, Indoors; Colour: black; IDs, certificates: VDE; Manufacturer's Warranty: 5 years; Version: black; PU1, EAN: 4007841081706

**Manufacturer** Steinel

**Prod. No.** 081706

**Ordering designation**

Deliver, install and set ready for operation