**STEINEL Professional Presence detector**

**IR Micro**

**DALI-2 Input Device**

Type: Presence detector; Dimensions (Ø x H): 80 x 21 mm; Mains power supply: 12 – 22,5 V; Power supply, detail: DALI bus; Number of Dali users: 2; Sensor Technology: passive infrared; Application, place: Indoors; Installation site: ceiling; Installation: Concealed wiring; Mounting height: 2,00 – 5,00 m; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 6 x 6 m (36 m²); Reach, presence: 4 x 4 m (16 m²); Detection angle: 360 °; Angle of aperture: 160 °; Switching zones: 168 switching zones; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: No; Twilight setting TEACH: No; Twilight setting: 2 – 1000 lx; Switching output 1, floating: No; Control output, Dali: Addressable/slave; Constant-lighting control: No; Basic light level function: No; Settings via: Bus; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave; IP-rating: IP20; Material: Plastic; Ambient temperature: 0 – 40 °C; Application, room: one-person office, hotel room, care room, function room / ancillary room, WC / washroom, Indoors; Colour: white; Colour, RAL: 9003; Manufacturer's Warranty: 5 years; Version: DALI-2 Input Device; PU1, EAN: 4007841057732

**Manufacturer** Steinel

**Prod. No.** 057732

**Ordering designation**

Deliver, install and set ready for operation