**STEINEL Professional Presence detector**

**IR Quattro MICRO**

**COM1 - black**

Type: Presence detector; Dimensions (Ø x H): 43 x 75 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,5 W; Sensor Technology: passive infrared; Application, place: Indoors; Installation site: ceiling; Installation: In-ceiling installation; Mounting height: 2,00 – 5,00 m; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 6 x 6 m (36 m²); Reach, presence: 4 x 4 m (16 m²); Detection angle: 360 °; Angle of aperture: 90 °; Switching zones: 168 switching zones; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: No; Twilight setting TEACH: Yes; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 60 min; Output: 1000 W; Switching output 1, resistive: 1000 W; Switching output 1, number of LEDs / fluorescent lamps: 8 pcs.; Switching output 1, floating: No; Fluorescent lamps, electronic ballast: 500 W; Fluorescent lamps, uncorrected: 400 VA; Fluorescent lamps, series-corrected: 400 VA; Fluorescent lamps, parallel-corrected: 400 VA; Switching output 1, low-voltage halogen lamps: 1000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 300 W; LED lamps > 8 W: 600 W; Capacitive load in μF: 176 µF; Constant-lighting control: No; Basic light level function: No; Settings via: Remote control, Smart Remote; With remote control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; IP-rating: IP65; Material: Plastic; Ambient temperature: -25 – 55 °C; Application, room: one-person office, hotel room, care room, function room / ancillary room, WC / washroom, Indoors; Colour: black; Colour, RAL: 9005; Manufacturer's Warranty: 5 years; Version: COM1 - black; PU1, EAN: 4007841068639

**Manufacturer** Steinel

**Prod. No.** 068639

**Ordering designation**

Deliver, install and set ready for operation