**STEINEL Professional Motion detector**

**IS 2360 ECO**

**white**

Type: Motion detectors; Dimensions (Ø x H): 115 x 51 mm; Mains power supply: 230 V / 50 – 60 Hz; Sensor Technology: passive infrared; Application, place: Outdoors, Indoors; Installation site: ceiling; Installation: Surface wiring; Mounting height: 2,00 – 4,00 m; Reach, radial: Ø 3 m (7 m²); Reach, tangential: Ø 7 m (38 m²); Detection angle: 360 °; Angle of aperture: 180 °; Switching zones: 664 switching zones; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Twilight setting TEACH: No; Twilight setting: 2 – 2000 lx; Time setting: 8 sec – 35 min; Output: 2000 W; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 6 pcs.; Fluorescent lamps, electronic ballast: 1500 W; Fluorescent lamps, uncorrected: 500 VA; Fluorescent lamps, series-corrected: 500 VA; Fluorescent lamps, parallel-corrected: 500 VA; Switching output 1, low-voltage halogen lamps: 1000 VA; LED lamps < 2 W: 16 W; LED lamps > 2 W < 8 W: 64 W; LED lamps > 8 W: 64 W; Capacitive load in μF: 132 µF; Constant-lighting control: No; Basic light level function: No; Settings via: Potentiometers; With remote control: No; Interconnection: Yes; Type of interconnection: Master/master; IP-rating: IP54; Material: Plastic; Ambient temperature: -20 – 50 °C; Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, WC / washroom, multi-storey / underground car park, outdoors, warehouse, Indoors; Colour: white; Colour, RAL: 9010; IDs, certificates: VDE; Manufacturer's Warranty: 5 years; Version: white; PU1, EAN: 4007841006556

**Manufacturer** Steinel

**Prod. No.** 006556

**Ordering designation**

Deliver, install and set ready for operation