**STEINEL Professional Multisensor**

**Multisensor Air KNX**

**V3.0**

Type: Other; Dimensions (L x W x H): 33 x 123 x 123 mm; Mains power supply: 30 V; Power consumption: 0,5 W; Power supply, detail: KNX bus; Sensor Technology: Multisensor; Application, place: Indoors; Installation site: ceiling; Installation: Concealed wiring; Mounting height: 4,00 m; Optimum mounting height: 2,8 m; Twilight setting TEACH: Yes; Twilight setting: 2 – 1000 lx; Constant-lighting control: No; Basic light level function: Yes; KNX functions: Comfort, CO2, Light level, HVAC output, Air pressure, Humidity output, Dewpoint, Temperature output, VOC, Photo-cell controller, Logic gate; With bus coupling: Yes; Settings via: ETS software, Bluetooth, Bus; With remote control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; IP-rating: IP20; Material: Plastic; Ambient temperature: 0 – 40 °C; Application, room: classroom, lecture hall, one-person office, open-plan office, conference room / meeting room, hotel room, care room, duty room, recreation room, sports hall, reception / lobby, Indoors; Colour: white; Colour, RAL: 9016; Manufacturer's Warranty: 5 years; PU1, EAN: 4007841056346

**Manufacturer** Steinel

**Prod. No.** 056346

**Ordering designation**

Deliver, install and set ready for operation