**STEINEL Professional Presence detector**

**Single US**

**DALI-2 Input Device**

Type: Presence detector; Dimensions (L x W x H): 71 x 120 x 120 mm; Mains power supply: 16 V; Power supply, detail: DALI bus; Number of Dali users: 10; Sensor Technology: Ultrasonic; Application, place: Indoors; Installation site: ceiling; Installation: Concealed wiring; Mounting height: 2,50 – 3,50 m; Reach, radial: 10 x 3 m (30 m²); Reach, tangential: 10 x 3 m (30 m²); Ultrasonic technology: 40 kHz; Detection angle: 180 °; Angle of aperture: 180 °; Optimum mounting height: 2,5 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Twilight setting TEACH: No; Twilight setting: 10 – 1000 lx; Control output, Dali: Addressable/slave; Constant-lighting control: No; Basic light level function: No; Settings via: Bus; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave; Material: Plastic; Ambient temperature: -25 – +55 °C; Application, room: corridor / aisle, stairwell, Indoors; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: DALI-2 Input Device; PU1, EAN: 4007841057503

**Manufacturer** Steinel

**Prod. No.** 057503

**Ordering designation**

Deliver, install and set ready for operation