**STEINEL Professional Presence detector**

**IR Quattro SLIM KNX**

**KNX V3**

Type: Presence detector; Dimensions (L x W x H): 55 x 77 x 77 mm; Power supply, detail: KNX bus; Sensor Technology: passive infrared; Application, place: Indoors; Installation site: ceiling; Installation: In-ceiling installation; Mounting height: 2,50 – 4 m; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 4 x 4 m (16 m²); Reach, presence: 4 x 4 m (16 m²); Reach, detail: Retina lens and hexagonal Fresnel structure; Detection angle: 360 °; Angle of aperture: 71 °; Switching zones: 260 switching zones; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: No; Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 10 sec – 1092 min; Constant-lighting control: No; Basic light level function: Yes; KNX functions: Photo-cell controller, Basic light level function, Light level, HVAC output, Constant-lighting control, Light output 4x, Presence output, Day / night function, Logic gate; With bus coupling: Yes; Settings via: ETS software, Remote control, Bus, Smart Remote; With remote control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; IP-rating: IP20; Material: Plastic; Ambient temperature: 0 – 40 °C; Application, room: one-person office, hotel room, care room, function room / ancillary room, WC / washroom, Indoors; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: KNX; PU1, EAN: 4007841058494

**Manufacturer** Steinel

**Prod. No.** 058494

**Ordering designation**

Deliver, install and set ready for operation