**STEINEL Professional Sensor-switched LED outdoor light**

**L 666 LED**

**Anthracite V2**

Dimensions (L x W x H): 122 x 102 x 269 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Mounting height max.: 2,50 m; Sensor Technology: passive infrared; Output: 8,5 W; Interconnection: Yes; Slave modeselectable: No; Luminous flux: 595 lm; Efficiency: 66 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Colour Rendering Index: 80-89; With lamp: Yes, STEINEL LED system; Lamp: LED cannot be replaced; LED life expectancy (max. °C): 50000 h; LED life expectancy (25 °C): > 60000 h; Base: without; LED cooling system: Passive Thermo Control; With motion detector: Yes; Detection angle: 360 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: r = 2 m (13 m²); Reach, tangential: r = 7 m (154 m²); Photo-cell controller: Yes; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Basic light level function time: 10/30 min, all night; Functions: 4 programme settings geared to practical needs, can be selected on removable sensor module; Soft light start: Yes; Continuous light: selectable, 4h; Impact resistance: IK07; IP-rating: IP44; Protection class: I; Ambient temperature: -20 – 50 °C; Housing material: Aluminium; Cover material: Plastic, opal; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; Cover material: shrouds; Version: Anthracite; PU1, EAN: 4007841053116

**Manufacturer** Steinel

**Prod. No.** 053116

**Ordering designation**

Deliver, install and set ready for operation