**STEINEL Professional Presence detector**

**True Presence**

**BT IPD (Slave) - surface**

Type: Presence detector; Dimensions (L x W x H): 45 x 123 x 123 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Sensor Technology: High frequency; Application, place: Indoors; Installation site: ceiling; Installation: Surface wiring; Mounting height: 2,00 – 12,00 m; Reach, radial: Ø 15 m (177 m²); Reach, tangential: Ø 15 m (177 m²); Reach, presence: Ø 15 m (177 m²); True Presence reach: Ø 9 m (64 m²); HF-system: 7,2 GHz; Detection angle: 360 °; Angle of aperture: 160 °; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Detection: also through glass, wood and stud walls; Twilight setting TEACH: No; Constant-lighting control: No; Basic light level function: No; Settings via: Bluetooth; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave; Material: Plastic; Ambient temperature: -20 – 50 °C; Application, room: classroom, lecture hall, one-person office, open-plan office, high-bay warehouse, production facilities, conference room / meeting room, hotel room, care room, duty room, recreation room, dining hall / staff restaurant, changing room, kitchenette, sports hall, reception / lobby, WC / washroom, warehouse, Indoors; Colour: white; Colour, RAL: 9003; Manufacturer's Warranty: 5 years; Version: BT IPD (Slave) - surface; PU1, EAN: 4007841064525

**Manufacturer** Steinel

**Prod. No.** 064525

**Ordering designation**

Deliver, install and set ready for operation