**STEINEL Professional Multisensor**

**True Presence Multisensor KNX**

**V3.0**

Type: Presence detector; Dimensions (L x W x H): 33 x 123 x 123 mm; Mains power supply: 30 V; Power consumption: 1 W; Power supply, detail: KNX bus; Sensor Technology: High frequency; Application, place: Indoors; Installation site: ceiling; Installation: Concealed wiring; Mounting height: 2,00 – 12,00 m; Reach, radial: Ø 15 m (177 m²); Reach, tangential: Ø 15 m (177 m²); Reach, presence: Ø 15 m (177 m²); True Presence reach: Ø 9 m (64 m²); HF-system: 7,2 GHz; Detection angle: 360 °; Angle of aperture: 160 °; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Detection: also through glass, wood and stud walls; Twilight setting TEACH: Yes; Twilight setting: 2 – 2000 lx; Time setting: 30 sec – 1092 min; Constant-lighting control: Yes; Basic light level function: Yes; KNX functions: Comfort, CO2, Photo-cell controller, Basic light level function, Light level, HVAC output, Constant-lighting control, Light output 4x, Air pressure, Humidity output, Presence output, Day / night function, Dewpoint, VOC, Temperature output, Logic gate; With bus coupling: Yes; Settings via: ETS software, Bluetooth, Bus; With remote control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; IP-rating: IP20; Material: Plastic; Ambient temperature: 0 – 40 °C; Application, room: classroom, lecture hall, one-person office, open-plan office, conference room / meeting room, hotel room, care room, duty room, recreation room, sports hall, reception / lobby, Indoors; Colour: white; Colour, RAL: 9003; Manufacturer's Warranty: 5 years; PU1, EAN: 4007841056353

**Manufacturer** Steinel

**Prod. No.** 056353

**Ordering designation**

Deliver, install and set ready for operation