**STEINEL Professional Accessory**

**eNet switching actuator**

Dimensions (Ø x H): 53 x 28 mm; Mains power supply: 230 V / 50 – 60 Hz; Installation site: wall, ceiling; Installation: Concealed wiring; With bus coupling: No; Settings via: eNet; IP-rating: IP00; Manufacturer's Warranty: 5 years; PU1, EAN: 4007841032838

**Manufacturer** Steinel

**Prod. No.** 032838

**Ordering designation**

Deliver, install and set ready for operation